---- TYPE_BLUECELL_ACK Matches (2 in 2 files) ----
RF_Status_Ack in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     Ack_Buf[INDEX_BLUE_TYPE]         = TYPE_BLUECELL_ACK;
zig_operate.h (D:\workspace\STM32F103_ATTEN_PLL_Zig\Inc) line 25 :     TYPE_BLUECELL_ACK    = 4,
