---- printf Matches (125 in 3 files) ----
Atten_PE43711_TraceValue_Func in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //   printf("\r\n ret : %f \r\n",ret);
Atten_Wifi_DataSet in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("ret :");
Atten_Wifi_DataSet in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //      printf("%02x ",buf[i]);
Atten_Wifi_DataSet in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\n");
PE43711_Ach_atten_ctrl in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : // printf("\r\n=================%d======0x%x=======\r\n",Ch,temp);
PE43711_Ach_atten_ctrl in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //      printf("1");
PE43711_Ach_atten_ctrl in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //      printf("0");
PE43711_Ach_atten_ctrl in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("\r\n==============================\r\n");
Uart_Data_Send in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("%02x ",data[i]);
Uart_Data_Send in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\n");
atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) line 1051 : uint8_t printf_if = 0;
Atten_Offset_QPC6614 in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         default : printf("Critical Error\r\n");
Atten_Offset_PE43711 in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         default : printf("Critical Error\r\n");
Atten_Offset_ADRF5720 in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         default : printf("Critical Error\r\n");
Atten_Offset_HMC939 in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         default : printf("Critical Error\r\n");
Atten_Operate in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("Last check ");
Atten_Operate in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //      printf("%02x ",data[i]);
Atten_Operate in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //              printf("%02x ",data[i]);
Atten_Operate in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("END \r\n");
Atten_Operate in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //                printf("%02x ",data[i]);
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("middle check ");
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //      printf("%02x ",data[i]);
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         printf("LINE : %d \r\n",__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :             default:printf("[Error ]Defalut in %s      LINE :%d \r\n",__func__,__LINE__);break;
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("middle check 2");
Atten_Operate_Mem_RW in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //      printf("%02x ",data[i]);
LCD_Button_Read in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("Button_ESC \r\n",__func__,__LINE__);
LCD_Button_Read in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("Button_MENU \r\n",__func__,__LINE__);
LCD_Button_Read in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("Button_UP \r\n",__func__,__LINE__);
LCD_Button_Read in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("Button_DOWN \r\n",__func__,__LINE__);
LCD_Button_Read in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //        printf("Button_ENTER \r\n",__func__,__LINE__);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("function %s LINE : %d\r\n",__func__,__LINE__);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\nAch_150M_Value : %06.2f \r\n",Ach_150M_Value);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\Atten_Setting.ATT_A_CH_WIFI2_4Ghz_PE43711_1 : %02x \r\n",Atten_Setting.ATT_A_CH_WIFI2_4Ghz_PE43711_1);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\Ach_Wifi_2_4GHz_Value : %06.2f \r\n",Ach_Wifi_2_4GHz_Value);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\Ach_Wifi_2_4GHz_Value : %06.2f \r\n",Ach_Wifi_2_4GHz_Value);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\Ach_Wifi_2_4GHz_Value : %06.2f \r\n",Ach_Wifi_2_4GHz_Value);
LCD_M68_DataWrite_COMMAND_Init in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("\r\ RES : Ach_Wifi_2_4GHz_Value : %06.2f \r\n",Ach_Wifi_2_4GHz_Value);
Character_Lcd_chMenu in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //                      printf("function %s LINE : %d\r\n",__func__,__LINE__);
Lcd_AchSetting_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    Setting");    
Lcd_Ach150M_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", Ach_150M_Value); 
Lcd_Ach150M_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("Ach_150M_Value : %f \r\n,",Ach_150M_Value);
Lcd_AchWifi_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", Ach_Wifi_2_4GHz_Value);    
Lcd_Ach30G_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", Ach_30G_28_28_5_Value);    
Lcd_BchSetting_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    Setting"); 
Lcd_Bch150M_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", Bch_150M_Value);    
Lcd_BchWifi_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", Bch_Wifi_2_4GHz_Value);    
Lcd_Bch30G_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", Bch_30G_28_28_5_Value);    
LCD_150M_ValueChange_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", *data);    
LCD_150M_ValueChange_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("data : %f   offset :  %f\r\n",*data,offset);
LCD_Wifi_ValueChange_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", *data);    
LCD_30G_ValueChange_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", *data);   
LCD_Wifi_Freq_Select_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", *db_value);    
LCD_30G_Freq_Select_Display in Character_lcd.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     sprintf(temp_str, "    %06.2f   dB", *db_value);    
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //    printf("%s  : %d \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("Button_PRESS ESC \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("Button_UnPRESS ESC \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //				printf("Button_PRESS MENU \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //				printf("Button_UNPRESS MENU \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("Button_UP UNPRESS \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //				printf("Button_UP PRESS \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("Button_DOWN UNPRESS \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //				printf("Button_DOWN PRESS \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("Button_ENTER PRESS \r\n",__func__,__LINE__);
HAL_GPIO_EXTI_Callback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("Button_ENTER UNPRESS \r\n",__func__,__LINE__);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     setbuf(stdout, NULL); // \n ?ï¿½ï¿½?ï¿½ï¿½?ï¿½ï¿½, printf ï¿??????ï¿½ï¿½?ï¿½ï¿½ï¿????? ?ï¿½ï¿½?ï¿½ï¿½?ï¿½ï¿½
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("PE43711_ATTEN_31_75DB_Trace  : %02x \r\n",PE43711_ATTEN_31_75DB_Trace);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("PE43711_ATTEN_16DB_Trace  : %02x \r\n",PE43711_ATTEN_16DB_Trace);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("PE43711_ATTEN_8DB_Trace  : %02x \r\n",PE43711_ATTEN_8DB_Trace);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("PE43711_ATTEN_4DB_Trace  : %02x \r\n",PE43711_ATTEN_4DB_Trace);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("PE43711_ATTEN_2DB_Trace  : %02x \r\n",PE43711_ATTEN_2DB_Trace);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //  printf("PE43711_ATTEN_1DB_Trace  : %02x \r\n",PE43711_ATTEN_1DB_Trace);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     printf("****************************************\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     printf("TEST Project\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     printf("Build at %s %s\r\n", __DATE__, __TIME__);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     printf("Copyright (c) 2019. BLUECELL\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     printf("****************************************\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : 				printf("%02x ",buf[i]);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //            printf("\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         				printf("%02x ",buf[i]);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :                 printf("\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :                 printf("CHECKSUM_ERROR  RecvCRC : %02x  , index %d\r\n",buf[3 + buf[Bluecell_Length]],5 + buf[Bluecell_Length]);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :                  printf("What Happen?\r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :                 printf("ButtonLong_TimerCnt \r\n");
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) : //                printf("LONG KEY PRESS\r\n");
assert_failed in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :      tex: printf("Wrong parameters value: file %s on line %d\r\n", file, line) */
